# Duct Calc
Duct sizing based on ACCA, Manual-D.
Keywords: duct, hvac, duct-design, duct design, manual-d, manual d, design

# Room Loads

Heating Total
42,255
Cooling Total
26,835
Cooling Sensible
22,273

# Sensible Heat Ratio

SHR

Name | Heating Load | Cooling Total | Cooling Sensible | Register Count | Delegated To |
--- | --- | --- | --- | --- | --- | ---

Bed-1

3,913

2,472

2,052

1

# Room

Name Level
Use -1 or 0 for a basement
Heating Load Cooling Total Cooling Sensible

Should enter at least one of the cooling loads.

Both are also acceptable.

Registers Room

Entry

8,284

2,916

2,420

2

# Room

Name Level
Use -1 or 0 for a basement
Heating Load Cooling Total Cooling Sensible

Should enter at least one of the cooling loads.

Both are also acceptable.

Registers Room

Family Room

9,785

7,446

6,180

3

# Room

Name Level
Use -1 or 0 for a basement
Heating Load Cooling Total Cooling Sensible

Should enter at least one of the cooling loads.

Both are also acceptable.

Registers Room

Kitchen

4,518

5,096

4,230

2

# Room

Name Level
Use -1 or 0 for a basement
Heating Load Cooling Total Cooling Sensible

Should enter at least one of the cooling loads.

Both are also acceptable.

Registers Room

Living Room

7,553

6,829

5,668

2

# Room

Name Level
Use -1 or 0 for a basement
Heating Load Cooling Total Cooling Sensible

Should enter at least one of the cooling loads.

Both are also acceptable.

Registers Room

Master

8,202

2,076

1,723

2

# Room

Name Level
Use -1 or 0 for a basement
Heating Load Cooling Total Cooling Sensible

Should enter at least one of the cooling loads.

Both are also acceptable.

Registers Room

# Room

Name Level
Use -1 or 0 for a basement
Heating Load Cooling Total Cooling Sensible

Should enter at least one of the cooling loads.

Both are also acceptable.

Registers Room

# Upload CSV

Drag and drop, or click to upload